How to install the SL-SLX Control Interface

All you need to do to install the GUI is to drag all of the following files in a single folder.
	-SL-SLX CONTROL INTERFACE (application file)
	-default.esi
	-last.esi
	-SL SLX Service Tool.esi
	-SL SLX  Service Tool - Set Show Position 2.esi
	-SL SLX Lift Commissioning Tool.esi

No further installation steps are necessary for the software to function.

Please Note: Make sure your computer's COM Port is configured to provide RS232 communications via the R2D7 RS232 bridge.
See your computer literature for details on how to do this, and use the information in the GUI instructions to
configure the COM port.